|  |
| --- |
| 1871 |
| **BULJAN CESTE d.o.o. Troska bb**  **71260 Kreševo, Bosnia and Herzegovina**  **20**  1871 – CPR – 0247 |
| **EN 12899-1:2007**  **bc-oz 60-1R**  Reinforced sign plate round φ 600 mm, with sign materials applied for fixed vertical road traffic signs, with bended edge  **Resistance to horizontal loads** -  Fixings – Pass (material – steel)  Wind action – WL9  Temporary deflection bending – TDB2  Dynamic snow load – DSL2  Point loads – PL1  Permanent deflection – Pass  Partial action factor – PAF1  **Visibility characteristics**  Daylight chromaticity & luminance factor – B1 & B2  Coefficient of retroreflection – RA1  **Durability**  Impact resistance of sign face material – Pass  Resistance to corrosion of sign plate – Aluminum, SP1 |