|  |
| --- |
| 1871 |
| **BULJAN CESTE d.o.o. Troska bb****71260 Kreševo, Bosnia and Herzegovina****20**1871 – CPR – 0247 |
| **EN 12899-1:2007****bc-tz 90-2R**Sign plate equilateral triangle 900x900x900 mm, with sign materials applied for fixed vertical road traffic signs, with double bended edges**Resistance to horizontal loads** -Fixings – Pass (material – steel)Wind action – WL6Temporary deflection bending – TDB1Dynamic snow load – DSL1Point loads – PL1Permanent deflection – PassPartial action factor – PAF1**Visibility characteristics**Daylight chromaticity & luminance factor – B1 & B2Coefficient of retroreflection – R2**Durability**Impact resistance of sign face material – PassResistance to corrosion of sign plate – Aluminum, SP1  |